&params_run
duration='4ts'
nb_proc_atm=15
nb_proc_oce=0
/
